For 1990-2009 cars

#### Special Tools

• | KM-470-B Angular Torque Gage

• | EN-48252 Crankshaft Oil Seal Installer

Notice: Refer to Fastener Notice in the Preface section.

1. Install the CPS target wheel.

Tighten
Tighten the CPS target wheel tightening bolts to 12 N·m (8.9 lb ft).

2. Install the oil nozzle tube.

Tighten
Tighten the oil nozzle tube retaining bolts to 23 N·m (17 lb ft).

Important: Check the crankshaft and main bearing for damages, scratches and foreign materials.

3. Lubricate the main bearings and crankshaft with new engine oil.
4. Install the main bearings on the original position.
5. Install the crankshaft.
6. Remove the lower crankcase. Refer to Lower Crankcase Replacement.
7. Install the crankshaft rear sealing with NEW one using by crankshaft rear oil seal installer EN-48252 .
8. Install the connecting rod caps. Refer to Piston, Connecting Rod, and Bearing Installation.
9. Assemble the engine block. Refer to Engine Block Disassemble.