For 1990-2009 cars

### Removal Procedure

1. Remove the front mud guards.
2. Remove the screws and front fender wheel opening molding.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front fender wheel opening molding with the screws.

Tighten
Tighten the front fender wheel opening molding screws to 4 N·m (35 lb in).

2. Install the front mud guard.