For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel storage compartment. Refer to Instrument Panel Storage Compartment Replacement .
2. Remove the screws and the instrument panel passenger molding.
3. Using a flat-bladed tool,remove the instrument panel passenger vent.

### Installation Procedure

1. Press the instrument panel passenger vent into the housing.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the Install the instrument panel passenger molding with the screws.

Tighten
Tighten the instrument panel molding screws to 2 N·m (18 lb in).

3. Install the instrument panel storage compartment. Refer to Instrument Panel Storage Compartment Replacement.