For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the accelerator pedal module (APM) connector locking tab from the APM connector.
3. Disconnect the APM connector.
4. Remove the bolts, three places, attaching the APM from the accelerator and brake pedal module bracket.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the APM retaining bolts to the accelerator and brake pedal module bracket and tighten to 9 N·m (80 lb in).
2. Connect the APM connector and the install the locking tab firmly.