For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

Important: Only lift the engine far enough to take the weight off the transaxle front mount assembly, or damage to the mount and lifting equipment failure may occur.

1. Support the engine assembly using DW-110-060 .
2. Remove the transaxle front mount-to-transaxle through bolt.
3. Remove the transaxle front mount retaining bolts from the transaxle.
4. Remove the transaxle front mount assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the transaxle front mount assembly.

Tighten
Tighten the transaxle front mount retaining bolts to 50 N·m (36.9 lb ft).

Important: Before tightening the transaxle front mount through bolt swing the engine assembly backwards and forwards or from the side to side for the proper alignment.

2. Install the transaxle front mount through bolt.

Tighten
Tighten the transaxle front mount-to-transaxle through bolt to 90 N·m (66 lb ft).

3. Remove the support fixture DW-110-060 .