For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

1. Remove the battery and battery tray. Refer to Battery Tray Replacement.
2. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.

Note: Only lift the engine far enough to take the weight off the transaxle front mount assembly, or damage to the mount and lifting equipment failure may occur.

3. Support the engine assembly using the DW-110-060 fixture .
4. Remove the transaxle mount bracket retaining bolts from the transaxle.
5. Remove the transaxle mount assembly retaining bolts from the left front longitudinal.
6. Remove the transaxle mount assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the transaxle mount assembly and tighten.

• | The transaxle mount assembly retaining bolts (2) to 37 N·m (27 lb ft).

• | The transaxle mount bracket retaining bolts (1) to 50 N·m (37 lb ft).

2. Remove DW-110-060 fixture .
3. Install the battery and battery tray. Refer to Battery Tray Replacement.
4. Install the engine dress cover. Refer to Fuel Injector Sight Shield Replacement.