For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Release the connector lock and pull the transducer wire connector out.
3. Remove the transducer with a wrench.
4. Discard the O-ring seal.

### Installation Procedure

1. Install the new O-ring seal on the transducer.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the pressure transducer.

Tighten
Tighten the pressure transducer to 7 N·m (62 lb in).

3. Connect the wire connector.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .