For 1990-2009 cars

### Removal Procedure

1. Remove the bolts from the left and right sides of the instrument panel (I/P) upper trim panel.
2. Remove the upper I/P trim panel from the instrument panel.

### Installation Procedure

1. Position the upper I/P trim panel to the instrument panel.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolts securing the sides of the upper I/P trim panel to the instrument panel and tighten to 2 N·m (18 lb in).