For 1990-2009 cars

Applications | Specifications
--- | ---
Sealants and Adhesives
Rear Main Bearing Cap | Three-Bond 1217F
Camshaft Carrier-to-Cylinder Head | HN 1581 (Loctite® 515)
Oil Pan Bolts | HN 1256 (Loctite® 542)
Oil Pump Bolts | HN 1256 (Loctite® 542)
Oil Pan Pickup Tube Bolts | HN 1256 (Loctite® 542)
Oil Gallery Plug | HN 1256 (Loctite® 542)
Coolant Jacket Caps and Plugs (Freeze Plugs) | HN 1756 (Loctite® 176)
Exhaust Manifold Studs/Nuts | Anti-Seize Compound
Lubricating System
Type | Forced Feed
Oil Pump Type | Rotary (Trochoid)
Oil Filter Type | Cartridge
Oil Pan Capacity (Including Oil Filter) | 4.5L
Engine Oil Type | API SL (ILSAC GF-III) grade SAE 5W-30 * Hot area : SAE 10W-30