For 1990-2009 cars

#### Special Tools

• | KM-470-B Angular Torque Gage

• | EN-48252 Crankshaft Oil Seal Installer

### Removal Procedure

1. Remove the engine assembly. Engine ReplacementRefer to
2. Seperate the engine from the transmission.
3. Remove the flywheel or flexible plate bolts.
4. Remove the flywheel or flexible plate.
5. Remove the rear main seal.

### Installation Procedure

1. Install the crankshaft rear rear main seal with new one using EN-48251 .
2. Install the flywheel or flexible plate.

Tighten
Tighten the flywheel or flexible plate tightening bolts to 105 N·m (77.4 lb ft).

3. Install the engine to the transmission.
4. Install the engine assembly. Refer to Engine Replacement.