For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Hold-Down Bar Bracket Retaining Nuts | 10 N·m | 89 lb in
Battery Tray Retaining Bolts | 10 N·m | 89 lb in
Engine Fuse Block Lower Cover Bolts | 10 N·m | 89 lb in
Engine Fuse Block Retaining Bolts | 3 N·m | 27 lb in
Generator Lower Support Bracket Bolts | 25 N·m | 18 lb ft
Generator-to-Generator Lower Support Bracket Through Bolt | 40 N·m | 30 lb ft
Generator-to-Intake Manifold Strap Bracket Bolts at Generator | 35 N·m | 26 lb ft
Generator-to-Intake Manifold Strap Bracket Bolts at Intake Manifold | 25 N·m | 18 lb ft
Generator Upper Bracket Bolts at Generator | 35 N·m | 26 lb ft
Generator Upper Bracket Bolts at Intake Manifold and Coolant Bypass Housing | 25 N·m | 18 lb ft
Starter-to-Engine Block Mounting Bolt | 75 N·m | 55 lb ft
Starter Solenoid Terminal-to-Battery Lead Wire Nut | 15 N·m | 11 lb ft
Starter Solenoid Terminal-to-Generator Lead Wire Nut | 15 N·m | 11 lb ft
Starter-to-Transmission Mounting Bolt | 75 N·m | 55 lb ft