For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Pry off the reading lamp lens by inserting a screwdriver into the recess along the edge of the lens.
3. Remove the screws and the reading lamp housing from the headliner.
4. Disconnect the electrical connector.
5. Remove the bulb.

### Installation Procedure

1. Install the replacement bulb.
2. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the reading lamp housing to the headliner with the screws and tighten to 2 N·m (18 lb in).
4. Press the reading lamp lens onto the housing.
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.