For 1990-2009 cars

### Removal Procedure

1. Support the engine.
2. Remove the battery tray. Refer to Battery Tray Replacement .
3. Remove the transmission mount to transmission bolts.
4. Remove the transmission mount to frame rail bolts.
5. Remove the mount from the engine.

### Installation Procedure

1. Position the transmission mount on the frame rail.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the transmission mount to frame rail bolts.

Tighten
Tighten the bolts to 37 N·m (27 lb ft).

3. Install the transmission mount to transmission bolts.

Tighten
Tighten the bolts to 55 N·m (41 lb ft).

4. Install the battery tray. Refer to Battery Tray Replacement .
5. Remove the engine support.