For 1990-2009 cars

### Removal Procedure

1. Disconnect the engine wiring harness electrical connector (1) from the mass air flow (MAF) sensor.
2. Remove the MAF sensor screws.
3. Remove the MAF sensor.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the MAF sensor.
2. Install the MAF sensor screws and tighten to 0.6 N·m (5 lb in).
3. Connect the engine wiring harness electrical connector (1) to the MAF sensor.