For 1990-2009 cars

## Evaporator Tube Replacement First Design

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the air inlet grille. Refer to Air Inlet Grille Panel Replacement .

1 | A/C Condenser Tube Assembly Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement .

3 | A/C Compressor and Condenser Hose Assembly Nut Tighten 9 N·m (80 lb in)
4 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement .

5 | A/C Evaporator Hose Assembly Clip Nut (Qty: 2) Tighten 9 N·m (80 lb in)
6 | A/C Evaporator Hose Assembly Bolt (Qty: 2) Tighten 16 N·m (12 lb ft)
7 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement .

8 | A/C Evaporator Hose Assembly

## Evaporator Tube Replacement Second Design

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the air inlet grille. Refer to Air Inlet Grille Panel Replacement .
3. Remove the A/C Condenser Tube Assembly from the Evaporator Tube. Refer to Compressor Hose Assembly Replacement.

1 | A/C Evaporator Hose Assembly Nut. Tighten 9 N·m (80 lb in)
2 | A/C Evaporator Hose Assembly Bolt. Tighten 9 N·m (80 lb in)
3 | Sealing Washer (Qty 2).

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement .

4 | A/C Evaporator Hose Assembly.