For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Fender Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tip First design vehicles have three fasteners along catwalk area. Second design has only two fasteners along catwalk area. Replacement parts reflect only second design fenders (two holes).

Tighten
2.5 N·m (22 lb in)

2 | Front Fender Retainer (Qty: 3)
3 | Front Fender Bolt (Qty: 1) Tighten 10 N·m (89 lb in)
4 | Front Fender Bolt (Qty: 4) Tighten 10 N·m (89 lb in)
5 | Front Fender Bolt (Qty: 1) Tighten 10 N·m (89 lb in)
6 | Front Fender