For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Remove the front door trim panel. Refer to Door Trim Panel Replacement .

1 | Front Side Door Check Link Bolt Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Support the door before removing the hinge bolts.

Tighten
10 N·m (89 lb in)

2 | Front Side Door Upper Hinge Bolt (Qty: 2)

#### Procedure

1. Remove the water deflector.
2. Support the door before removing the hinge bolts.
3. Disconnect the electrical connector, if equipped.
4. With the aid of an assistant, remove the door.

Tighten
30 N·m (22 lb ft)

3 | Front Side Door Lower Hinge Bolt (Qty: 2) Tighten 30 N·m (22 lb ft)
4 | Front Side Door Assembly

#### Procedure

When replacing the door it is necessary to transfer all of the internal components.