For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the 3 hold down bolts for the underhood electrical center and position aside. Refer to Underhood Electrical Center or Junction Block Replacement .
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .

1 | Air Inlet Housing Nuts (Qty: 5) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Air Inlet Housing Front Panel Assembly