For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the radiator air upper baffle and deflector. Refer to Radiator Air Upper Baffle and Deflector Replacement .
2. Remove the charge air cooler inlet pipe. Refer to Charge Air Cooler Inlet Pipe Replacement .
3. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement .
4. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
5. Remove the air cleaner duct. Refer to Air Cleaner Outlet Duct Replacement .

1 | Radiator Assembly Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Cooling Fan and Motor Shroud Assembly

#### Procedure

Disconnect the cooling fan motor electrical connector.