For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel left closeout/insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
2. Remove the clutch master cylinder push rod (1) from the clutch pedal arm integral stud.
3. Remove the clutch pedal position switches. Refer to Clutch Pedal Position Switch Replacement.
4. Remove the clutch pedal bracket to cowl nut (5).
5. Remove the clutch pedal bracket to cowl bolt (4).
6. Remove the clutch pedal bracket to cowl nuts (2).
7. Remove the clutch pedal assembly (1).

### Installation Procedure

1. Install the clutch pedal assembly (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the clutch pedal bracket to cowl nuts (2).

Tighten
Tighten the nuts to 10 N·m (89 in lb).

3. Install the clutch pedal bracket to cowl bolt (4).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Install the clutch pedal bracket to cowl nut (5).

Tighten
Tighten the nut to 10 N·m (89 lb in).

5. Install the clutch pedal position switches. Refer to Clutch Pedal Position Switch Replacement.
6. Install the clutch master cylinder push rod (1) to the clutch pedal arm integral stud.
7. Install the instrument panel left closeout/insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.