For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the stabilizer shaft from the stabilizer shaft link. Refer to Stabilizer Shaft Link Replacement .

1 | Stabilizer Shaft Mounting Bolts (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 55 N·m (41 lb ft)
2 | Stabilizer Shaft Mounting Bracket
3 | Front Stabilizer Shaft Tip Remove the insulators from the stabilizer shaft.