For 1990-2009 cars

### Removal Procedure

1. Remove the hood. Refer to Hood Replacement .
2. Remove the horn. Refer to Horn Replacement .
3. Remove the charge air cooler inlet pipe bolt (3) at the rear bracket.
4. Remove the charge air cooler rear bracket nut (2) and bracket (1).
5. Remove the charge air cooler inlet pipe bolt (1) at the front bracket.
6. Loosen the charge air cooler clamp (2) at the charge air cooler inlet pipe.
7. Loosen the charge air cooler inlet pipe clamp (4) at the charge air cooler pipe.
8. Remove the charge air cooler inlet pipe.
9. Remove any oil film from inside the pipes.

### Installation Procedure

1. Install the charge air cooler inlet pipe to the charge air cooler pipe and the charge air cooler.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the charge air cooler rear bracket (1) and nut (2).

Tighten
Tighten the nut to 9 N·m (80 lb in).

3. Install the charge air cooler inlet pipe bolt (3) at the rear bracket.

Tighten
Tighten the bolt to 7 N·m (62 lb in).

4. Install the charge air cooler inlet pipe bolt (1) at the front bracket.

Tighten
Tighten the bolt to 7 N·m (62 lb in).

5. Tighten the charge air cooler clamp (2) at the charge air cooler pipe.
6. Tighten the charge air cooler inlet pipe clamp (4) at the charge air cooler pipe.

Tighten
Tighten the clamps to 5 N·m (44 lb in).

7. Install the horn. Refer to Horn Replacement .
8. Install the hood. Refer to Hood Replacement .