For 1990-2009 cars

## Front Fender Emblem/Nameplate Replacement GME

Callout | Component Name
--- | ---
1 | Front Fender Emblem Assembly Tip When removing protective liners from adhesive backed emblems, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.

#### Procedure

1. Use a J 25070 Heat Gun or equivalent to remove the old emblem. Clean all the adhesive residue from the fender, wipe the surface dry with a clean lint-free towel prior to installing new emblem.
2. Apply thumb pressure to the emblem to ensure full adhesion is made to the fender.

## Front Fender Emblem/Nameplate Replacement GT

Callout | Component Name
--- | ---
1 | Front Fender Emblem Assembly Caution: Refer to Exterior Trim Emblem Removal Caution in the Preface section.

#### Procedure

1. Use a J 25070 Heat Gun or equivalent to remove the old emblem.
2. Clean all the adhesive residue from the fender, wipe the surface dry with a clean lint-free towel prior to installing new emblem.
3. Callout (a) 2.09 in (53.3 mm) from the top side of the fender edge to the top of the emblem.
4. Callout (b) 2.33 in (59.1 mm) to the rear edge of the "T" on the GT emblem.
5. Apply palm pressure to the emblem to ensure full adhesion is made to the fender.
6. Clean any residue from the fender panel after emblem installation.