For 1990-2009 cars

The following service procedures require either a programming or a setup event be performed for a complete repair.

### ECM Replacement

1. If the engine control module (ECM) is replaced, the ECM Reprogramming procedure must be performed. Refer to Service Programming System (SPS).
2. Clutch Pedal Position Sensor Learn--Refer to Clutch Pedal Position Sensor Learn.

### ECM Reprogramming

If the ECM needs to be reprogrammed, refer to Service Programming System (SPS).