For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the charge air cooler inlet pipe. Refer to Charge Air Cooler Inlet Pipe Replacement.
3. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement.
4. Remove the lower radiator air baffle. Refer to Radiator Air Lower Baffle and Deflector Replacement.
5. Remove the upper radiator air baffle. Refer to Radiator Air Upper Baffle and Deflector Replacement.

1 | A/C Condenser Tube Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

3 | A/C Compressor and Condenser Hose Nut Tighten 9 N·m (80 lb in)
4 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement.

5 | A/C Condenser Bolt Tighten 9 N·m (80 lb in)
6 | Radiator Assembly Bolt Tighten 25 N·m (18 lb ft)
7 | Receiver Dehydrator Assembly Bolt Tighten 6 N·m (53 lb in)
8 | Receiver Dehydrator Assembly Bolt Tighten 6 N·m (53 lb in)
9 | O-Ring

#### Procedure

Remove and discard O-rings.

10 | A/C Receiver Dehydrator Assembly
11 | A/C Condenser Assembly