For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the charge air cooler inlet pipe if equipped. Refer to Charge Air Cooler Inlet Pipe Replacement .
2. Remove the charge air cooler outlet pipe if equipped. Refer to Charge Air Cooler Outlet Pipe Replacement .
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .

1 | Radiator Air Deflector Bolt - Front (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Radiator Air Deflector Assembly - Front
3 | Air Inlet Shroud Retainer (Qty: 2)
4 | Air Inlet Shroud