For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the door sill trim. Refer to Door Sill Plate Replacement .
2. Remove the lock pillar trim panel. Refer to Body Lock Pillar Trim Panel Replacement .
3. Remove the rear window panel trim. Refer to Rear Window Panel Trim Replacement .
4. Remove front floor console. Refer to Front Floor Console Replacement .
5. Remove front floor lower console. Refer to Front Floor Lower Console Replacement .
6. Remove front floor lower console cover. Refer to Front Floor Console Front Cover Replacement .

1 | Floor Panel Tunnel Carpet

#### Procedures

1. Replacement carpets will have perforations to allow tear off of the area to be removed.
2. Using the replacement carpet as a guide, cut the old carpet in front of the cross car beam and as high up the sides as possible in order to replace it without removing the HVAC module.
3. The passenger side of the carpet is to be tucked under HVAC unit.

2 | Floor Panel Tunnel Carpet "Service Only" Fastener

#### Procedure

Install the modified carpet with the supplied rivets approximately 115 mm (4.5 in) from the driver side cowl and 300 mm (11.8 in) up from the driver side floor pan sheet metal.