For 1990-2009 cars

### Tools Required

• | J 43276 Clutch Pilot Bearing Remover

• | J 38836 Pilot Bushing Installer/Clutch

### Removal Procedure

1. Remove the clutch. Refer to Clutch Pressure and Driven Plate Replacement .

Important: When using the J 43276, always secure the J 43276-1 tool body using a wrench. Do not allow the J 43276-1 tool to rotate. Failing to do so causes damage to the J 43276-1 tool body.

2. Remove the clutch bearing using the J 43276 .

2.1. | Install the J 43276-1 into the clutch pilot bearing .

2.2. | Using a wrench, secure the J 43276-1.

2.3. | Insert the J 43276-2 into the J 43276-1.

2.4. | Rotate the J 43276-2 clockwise into the J 43276-1 until the clutch pilot bearing is completely removed from the crankshaft.

2.5. | Rotate the J 43276-2 counterclockwise to remove the J 43276-2 from the J 43276-1.

2.6. | Remove the J 43276-1 from the tool body.

### Installation Procedure

1. Install a 5/8 inch washer (1) onto the J 38836 or equivalent. The washer serves as a stop against the crankshaft face and will assist in installing the bearing to the proper depth.
2. Install the new pilot bearing (2) onto the tool.
3. Install a new pilot bearing into the crankshaft using the J 38836 .
4. Inspect the clutch pilot bearing for proper installation. A properly installed clutch pilot bearing will be installed until flush to the rear of the crankshaft.
5. Install the clutch. Refer to Clutch Pressure and Driven Plate Replacement .