For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear compartment lid. Refer to Rear Compartment Lid Replacement .
2. Remove the rear compartment torque rod. Refer to Rear Compartment Lid Hinge Torque Rod Replacement .

1 | Rear Compartment Lid Hinge Bolts (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 25 N·m (19 lb ft)
2 | Rear Compartment Hinge