For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Loosen the front and rear weatherstrip retainer one at a time. Refer to Folding Top Side Front Weatherstrip Retainer Replacement and Folding Top Side Rear Weatherstrip Retainer Replacement .

1 | Folding Top Side Front/Rear Weatherstrip Retainer

#### Procedure

Adjust the front retainer to the rear retainer (a), or the rear retainer to the front retainer (a), to 23.8 mm (1.067 in).

Tip
Do not remove both retainers at the same time.