For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the charge air cooler inlet pipe. Refer to Charge Air Cooler Inlet Pipe Replacement .
3. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement .
4. Remove the lower radiator air baffle. Refer to Radiator Air Lower Baffle and Deflector Replacement .
5. Remove the upper radiator air baffle. Refer to Radiator Air Upper Baffle and Deflector Replacement .

1 | A/C Condenser Tube Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement .

3 | A/C Compressor and Condenser Hose Nut Tighten 9 N·m (80 lb in)
4 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement .

5 | A/C Condenser Bolt Tighten 9 N·m (80 lb in)
6 | Radiator Assembly Bolt Tighten 25 N·m (18 lb ft)
7 | Receiver Dehydrator Assembly Bolt Tighten 6 N·m (53 lb in)
8 | Receiver Dehydrator Assembly Bolt Tighten 6 N·m (53 lb in)
9 | O-Ring

#### Procedure

Remove and discard O-rings.

10 | A/C Receiver Dehydrator Assembly
11 | A/C Condenser Assembly