For 1990-2009 cars

Table 1: | Indicators
Table 2: | Driver Information Center

#### Indicators

Symbol | Reference
--- | ---
| ABS: ABS Description and Operation.
| Air Bag: SIR System Description and Operation.
(Export) BRAKE | Brake: Brake Warning System Description and Operation.
| Charge: Charging System Description and Operation.
| Engine Coolant Temperature: Cooling System Description and Operation.
| The IPC illuminates the engine oil pressure (EOP) indicator when the engine control module (ECM) detects the EOP is low from the EOP sensor/switch.
| Front Fog Lamps: Exterior Lighting Systems Description and Operation
| High Beam: Exterior Lighting Systems Description and Operation.
| MIL: Engine Control Module Description
| Rear Fog Lamps: Exterior Lighting Systems Description and Operation
| Seat Belt: Seat Belt System Description and Operation.
| Security: Content Theft Deterrent (CTD) Description and Operation
| VDC: ABS Description and Operation
| Turn Signals: Exterior Lighting Systems Description and Operation.

#### Driver Information Center

Message | Reference
--- | ---
AUTO LIGHTS OFF | Exterior Lighting Systems Description and Operation.
AUTO LIGHTS ON | Exterior Lighting Systems Description and Operation.
BATTERY SAVER ACTIVE | Charging System Description and Operation.
BRAKE | Brake Warning System Description and Operation.
CHARGING SYSTEM ACTIVE | Charging System Description and Operation.
CHANGE OIL SOON | The driver information center (DIC) displays this message when the engine control module (ECM) determines that the engine oil life is 0 percent.
CHECK GAS CAP | Evaporative Emission Control System Description
DOOR AJAR | Door Ajar Indicator Description and Operation
ICE POSSIBLE | The driver information center (DIC) displays this message when the outside air temperature drops below 2°C (36°F). When the temperature rises above 5.5°C (42°F), the ICE POSSIBLE message turns OFF.
KEY FOB BATT LOW | Keyless Entry System Description and Operation.
LOW COOLANT | Cooling System Description and Operation.
LOW FUEL | The ECM monitors the fuel level sensor signal and will request the this message displayed when the fuel level value is less than 14 percent.
LOW OIL LEVEL | The DIC displays this message when the engine control module (ECM) detects a low oil level condition from the engine oil level sensor/switch.
LOW WASHER FLUID | Wiper/Washer System Description and Operation
POWER STEERING | Power Steering System Description and Operation.
REDUCED ENGINE POWER | Throttle Actuator Control (TAC) System Description
SERVICE AIR BAG | SIR System Description and Operation.
SERVICE VEHICLE SOON | The instrument panel cluster (IPC) displays the Service Vehicle Soon indicator when the BCM detects certain malfunctions that are not emissions related.
STARTING DISABLED | Starting System Description and Operation.
TRUNK AJAR | Luggage Compartment Description and Operation