For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Reposition the folding top side rear weatherstrip. Refer to Folding Top Side Rear Weatherstrip Replacement.
2. Remove the folding top side rear weatherstrip retainer. Refer to Folding Top Side Rear Weatherstrip Retainer Replacement.

1 | Folding Top Rear Locating Nut Caution: Refer to Fastener Caution in the Preface section. Tip Reposition the top cover for access to the nut retaining the locating pin. Tighten
3 N·m (26 lb in)

2 | Folding Top Rear Locating Pin

#### Procedure

Install a new locating pin.