For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the instrument panel (I/P) upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .

1 | Side Window Defogger Outlet Grille - RH

#### Procedure

Squeeze the tabs on the back of the outlet grille to release it from the trim panel.

2 | Side Window Defogger Outlet Grille - LH

#### Procedure

Squeeze the tabs on the back of the outlet grille to release it from the trim panel.