For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.
2. Remove the instrument panel compartment frame. Refer to Instrument Panel Compartment Door Opening Frame Replacement.
3. Remove the knee bolster assembly. Refer to Knee Bolster Replacement.

1 | Instrument Panel Lower Trim Panel Screw (Qty: 1) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Instrument Panel Lower Trim Panel Assembly

#### Procedures

1. Disconnect the electrical connections.
2. When replacing the instrument lower trim panel, transfer all necessary components.

3 | Retainer Clip (Qty: 6)