For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement .
3. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .

1 | Radiator Inlet Hose Assembly

#### Procedure

Using J 38185 position radiator inlet hose clamps aside and remove hose from the fittings.

#### Special Tools

J 38185 Hose Clamp Pliers