For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Reposition the folding top side rear weatherstrip. Refer to Folding Top Side Rear Weatherstrip Replacement .
2. Remove the folding top side rear weatherstrip retainer. Refer to Folding Top Side Rear Weatherstrip Retainer Replacement .

1 | Folding Top Rear Locating Nut Notice: Refer to Fastener Notice in the Preface section. Tip Reposition the top cover for access to the nut retaining the locating pin. Tighten
3 N·m (26 lb in)

2 | Folding Top Rear Locating Pin

#### Procedure

Install a new locating pin.