For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Brake Fluid Irritant Caution in the Preface section. Caution: Refer to Brake Dust Caution in the Preface section.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation .

1 | Brake Hose Fitting Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 40 N·m (30 lb ft)
2 | Brake Hose Fitting Gasket (Qty: 2) Tip DO NOT reuse the brake hose fitting gaskets. Install NEW gaskets.
3 | Front Brake Hose Tip Plug the brake hose fitting to prevent brake fluid loss and contamination.
4 | Brake Caliper Guide Pin Bolt (Qty: 2) Tighten: 34 N·m (25 lb ft)
5 | Brake Caliper Tip

1. If any of the disc brake caliper hardware is found to have excessive wear, replace to the hardware. Refer to Front Disc Brake Hardware Replacement .
2. Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding .
3. After the installation is complete and with the engine OFF, gradually apply the brake pedal to approximately 2/3 of its travel distance.
4. Slowly release the brake pedal.
5. Wait 15 seconds, then repeat steps 3-4 until a firm brake pedal is obtained. This will properly seat the brake caliper piston and the brake pads.
6. Fill the master cylinder to the proper level. Refer to Master Cylinder Reservoir Filling .
7. Burnish the pads and rotors. Refer to Brake Pad and Rotor Burnishing .