For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the transmission. Refer to Transmission Replacement .
3. Remove the clutch hose from the actuator cylinder. Refer to Hydraulic Clutch Hose/Pipe Replacement .

1 | Clutch Actuator Cylinder Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Use LOCTITE 592® P/N 21485278 thread sealant on the screws.

Tighten
10 N·m (89 lb in)

2 | Clutch Actuator Cylinder