For 1990-2009 cars

Callous | Component Name
--- | ---
Caution: Secure the steering wheel utilizing a strap to prevent rotation. Locking of the steering column will prevent damage and a possible malfunction of the SIR system. The steering wheel must be secured in position before disconnecting the following components:

• | The steering column

• | The intermediate shaft

• | The steering gear

After disconnecting these components, do not move the front tires and wheels. Failure to follow these procedures may cause improper alignment of some components during installation and result in possible damage to the SIR coil.

#### Preliminary Procedures

1. Remove the driver knee bolster bracket. Refer to Driver Knee Bolster Bracket Replacement.
2. If equiped, remove the clutch pedal. Refer to Clutch Pedal Replacement.
3. Remove the steering wheel. Refer to Steering Wheel Replacement.
4. Remove the steering column trim covers. Refer to Steering Column Trim Cover Replacement.

1 | Ignition/Start Switch Electrical Connector
2 | Intermediate Steering Shaft Bolt Caution: Refer to Fastener Caution in the Preface section. Tip Discard the bolt. Tighten
58 N·m (43 lb ft)

3 | Intermediate Steering Shaft Nut Tighten 58 N·m (43 lb ft)
4 | Steering Column Lower Support Bracket Bolt Tighten 25 N·m (18 lb ft)
5 | Steering Column Upper Support Bracket Nut (Qty: 2) Tighten 25 N·m (18 lb ft)
6 | Steering Column

#### Procedure

1. Disconnect all electrical connectors as needed.
2. Transfer any parts as needed.