For 1990-2009 cars

Connector 1: | X100 Engine Harness to the I/P Body Harness
Connector 2: | X102 Right Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness
Connector 3: | X103 Left Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness
Connector 4: | X110 Forward Lamp Harness to Left Headlamp Assembly Harness
Connector 5: | X111 Forward Lamp Harness to Right Headlamp Assembly Harness
Connector 6: | X120 Instrument Panel Body Harness to the Forward Lamp Harness
Connector 7: | X122 Forward Lamp Harness to the Outside Air Temperature Sensor Harness
Connector 8: | X162 Engine Harness to the Fuel Injector Jumper Harness
Connector 9: | X208 SIR I/P Module Harness to the I/P Body Harness
Connector 10: | X216 I/P Body Harness to the HVAC Harness
Connector 11: | X218 I/P Body Harness to the HVAC Harness
Connector 12: | X316 I/P Body Harness to the Passenger Seat Harness
Connector 13: | X317 I/P Body Harness to the Driver Seat Harness
Connector 14: | X400 I/P Body Harness to the Right Rear Lamp Assembly Harness
Connector 15: | X405 Rear Chassis Harness to Left Rear Lamp Assembly Harness
Connector 16: | X406 I/P Body Harness to Chassis Harness
Connector 17: | X407 Rear Chassis Harness to Right Rear Lamp Assembly Harness
Connector 18: | X408 Chassis Harness to I/P Body Harness
Connector 19: | X409 Chassis Harness to I/P Body Harness
Connector 20: | X410 I/P Body Harness to the Rear Lamp Jumper Harness
Connector 21: | X500 Driver Door Harness to the I/P Body Harness
Connector 22: | X501 Driver Door Harness to the I/P Body Harness (A31)
Connector 23: | X505 Driver Door Harness to the Power Mirror Jumper Harness
Connector 24: | X600 Passenger Door Harness to the I/P Body Harness

### X100 Engine Harness to the I/P Body Harness

#### Connector Part Information

- OEM: 15443822
- Description: 40-Way F GT 150 280 Series Sealed 4.0 5.2 (BK)

#### Connector Part Information

- OEM: 15317380
- Description: 40-Way M GT 150 280 Series Sealed (BK)

#### X100 Engine Harness to the I/P Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.5 WH | 1310 | Evaporative Emission (EVAP) Canister Vent Solenoid Control | A1 | 0.5 WH | 1310 | Evaporative Emission (EVAP) Canister Vent Solenoid Control
A2 | 0.5 RD/WH | 840 | Battery Positive Voltage | A2 | 0.5 RD/WH | 840 | Battery Positive Voltage
A3 | 0.35 TN | 1274 | 5-Volt Reference 3 | A3 | 0.35 TN | 1274 | 5-Volt Reference 3
A4 | 1.0 PU | 92 | Windshield Wiper Motor High Speed | A4 | 1.0 PU | 92 | Windshield Wiper Motor High Speed
A5 | 1.0 D-GN | 95 | Windshield Washer Switch Signal | A5 | 1.0 D-GN | 95 | Windshield Washer Switch Signal
A6-A7 | -- | -- | Not Used | A6-A7 | -- | -- | Not Used
A8 | 0.35 BN | 4 | Accessory Voltage | A8 | 0.35 BN | 4 | Accessory Voltage
B1 | 0.35 BN/WH | 419 | MIL Control | B1 | 0.35 BN/WH | 419 | MIL Control
B2 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+) | B2 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
B3 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-) | B3 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
B4-B5 | -- | -- | Not Used | B4-B5 | -- | -- | Not Used
B6 | 0.35 PU | 1272 | Low Reference | B6 | 0.35 PU | 1272 | Low Reference
B7 | 1.0 BK | 250 | Ground | B7 | 1.0 BK | 250 | Ground
B8 | 0.35 L-BU | 1162 | Throttle Position Sensor 2 Signal | B8 | 0.35 L-BU | 1162 | Throttle Position Sensor 2 Signal
B9 | 0.35 WH/BK | 1164 | 5-Volt Reference 2 | B9 | 0.35 WH/BK | 1164 | 5-Volt Reference 2
B10 | 0.35 BN | 1271 | Low Reference | B10 | 0.35 BN | 1271 | Low Reference
B11 | 0.35 D-BU | 1161 | Adjustable Accelerator Pedal Position (APP) Sensor 1 Signal | B11 | 0.35 D-BU | 1161 | Adjustable Accelerator Pedal Position (APP) Sensor 1 Signal
B12 | 0.5 TN | 2759 | Low Reference | B12 | 0.5 TN | 2759 | Low Reference
C1 | 0.5 PU | 1589 | Fuel Level Sensor Signal | C1 | 0.5 PU | 1589 | Fuel Level Sensor Signal
C2 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal | C2 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
C3 | 0.5 GY | 2709 | 5-Volt Reference 1 | C3 | 0.5 GY | 2709 | 5-Volt Reference 1
C4 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control | C4 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control
C5 | 0.5 YE | 196 | Windshield Wiper Motor Park Switch Signal | C5 | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal
C6 | 0.5 PK/BK | 5291 | Ignition 1 Voltage | C6 | 0.5 PK/BK | 5291 | Ignition 1 Voltage
C7 | 0.5 PK | 849 | Brake Fluid Level Sensor Signal | C7 | 0.35 PK | 849 | Brake Fluid Level Sensor Signal
C8-C12 | -- | -- | Not Used | C8-C12 | -- | -- | Not Used
D1 | 0.35 OG/D-GN | 7360 | Manual Transmission Clutch Position Sensor Return (MA5) | D1 | 0.35 OG/D-GN | 7360 | Manual Transmission Clutch Position Sensor Return (MA5)
D2 | 0.35 D-BU/WH | 7361 | Manual Transmission Clutch Position Sensor Supply (MA5) | D2 | 0.35 D-BU/WH | 7361 | Manual Transmission Clutch Position Sensor Supply (MA5)
D3 | 0.35 L-GN | 6338 | Manual Transmission Clutch Position Sensor Signal Position (MA5) | D3 | 0.35 L-GN | 6338 | Manual Transmission Clutch Position Sensor Signal Position (MA5)
D4-D5 | -- | -- | Not Available | D4-D5 | -- | -- | Not Available
D6 | 0.5 L-GN | 1478 | Coolant Level Switch Signal | D6 | 0.5 L-GN | 1478 | Coolant Level Switch Signal
D7 | 0.5 OG | 228 | Windshield Washer Pump Control | D7 | 0.35 OG | 228 | Windshield Washer Pump Control
D8 | -- | -- | Not Used | D8 | -- | -- | Not Used

### X102 Right Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 12186568
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12186271
- Description: 4-Way M Metri-Pack 150 Series Sealed (GY)

#### X102 Right Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-BU | 15 | Right Turn Signal Lamp Supply Voltage | A | 0.5 L-BU | 15 | Right Turn Signal Lamp Supply Voltage
B | 0.5 BN | 9 | Park Lamp Supply Voltage | B | 0.5 BN | 9 | Park Lamp Supply Voltage
C | 0.8 PK | 2234 | Front Fog Lamp Supply Voltage (T96) | C | 0.8 PK | 2234 | Front Fog Lamp Supply Voltage (T96)
D | 0.8 BK | 250 | Ground | D | 0.8 BK | 250 | Ground

### X103 Left Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 12186568
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12186271
- Description: 4-Way M Metri-Pack 150 Series Sealed (GY)

#### X103 Left Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-BU | 14 | Left Turn Signal Lamp Supply Voltage | A | 0.5 L-BU | 14 | Left Turn Signal Lamp Supply Voltage
B | 0.5 BN | 9 | Park Lamp Supply Voltage | B | 0.5 BN | 9 | Park Lamp Supply Voltage
C | 0.8 PU | 2234 | Front Fog Lamp Supply Voltage (T96) | C | 0.8 PU | 2234 | Front Fog Lamp Supply Voltage (T96)
D | 0.8 BK | 150 | Ground | D | 0.8 BK | 150 | Ground

### X110 Forward Lamp Harness to Left Headlamp Assembly Harness

#### Connector Part Information

- OEM: 15326815
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15369319
- Description: 4-Way M GT 150 Series Sealed (BK)

#### X110 Forward Lamp Harness to Left Headlamp Assembly Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage | A | 0.8 BK | -- | Left Headlamp High Beam Supply Voltage
B | 0.8 BK | 150 | Ground | B | 0.8 BK | -- | Ground
C | 0.8 YE | 712 | Left Headlamp Low Beam Supply Voltage | C | 0.8 RD | -- | Left Headlamp Low Beam Supply Voltage
D | 0.8 BK | 150 | Ground | D | 0.8 RD | -- | Ground

### X111 Forward Lamp Harness to Right Headlamp Assembly Harness

#### Connector Part Information

- OEM: 15326815
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15369319
- Description: 4-Way M GT 150 Series Sealed (BK)

#### X111 Forward Lamp Harness to Right Headlamp Assembly Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage | A | 0.8 BK | -- | Right Headlamp High Beam Supply Voltage
B | 0.8 BK | 250 | Ground | B | 0.8 BK | -- | Ground
C | 0.8 TN/WH | 312 | Right Headlamp Low Beam Supply Voltage | C | 0.8 RD | -- | Right Headlamp Low Beam Supply Voltage
D | 0.8 BK | 250 | Ground | D | 0.8 RD | -- | Ground

### X120 Instrument Panel Body Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 15326084
- Description: 16-Way F GT 150 280 Series Sealed 4.0 5.8 (BK)

#### Connector Part Information

- OEM: 15326085
- Description: 16-Way M GT 150 280 Series Sealed 4.0 5.8 (BK)

#### X120 Instrument Panel Body Harness to the Forward Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 PK/BK | 6434 | Can Bus High Serial Data (LNF) | A | 0.5 PK/BK | 6434 | Can Bus High Serial Data (LNF)
B | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal (JL9) | B | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal (JL9)
C | 0.5 OG | 885 | Low Reference (JL9) | C | 0.5 OG | 885 | Low Reference (JL9)
D | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal (JL9) | D | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal (JL9)
E | 0.5 WH | 883 | Low Reference (JL9) | E | 0.5 WH | 883 | Low Reference (JL9)
F | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+) | F | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
G | 0.5 TN | 2501 | High Speed GMLAN Serial Data (-) | G | 0.5 TN | 2501 | High Speed GMLAN Serial Data (-)
H | 0.5 D-GN | 2087 | Combined Vehicle Inertial Sensor Supply Voltage (LNF) | H | 0.5 D-GN | 2087 | Combined Vehicle Inertial Sensor Supply Voltage (LNF)
J | 0.5 L-BU | 2088 | Low Reference (LNF) | J | 0.5 L-BU | 2088 | Low Reference (LNF)
K | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+) | K | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
L | 0.5 TN | 2501 | High Speed GMLAN Serial Data (-) | L | 0.5 TN | 2501 | High Speed GMLAN Serial Data (-)
M | 0.5 YE/BK | 2160 | Front End Discriminating Sensor Signal | M | 0.5 YE/BK | 2160 | Front End Discriminating Sensor Signal
N | 0.5 GY | 5600 | Low Reference | N | 0.5 GY | 5600 | Low Reference
P | 0.5 YE | 1834 | Forward Discriminating Sensor Signal | P | 0.5 YE | 1834 | Forward Discriminating Sensor Signal
R | 0.5 TN/OG | 5045 | Low Reference | R | 0.5 TN/OG | 5045 | Low Reference
S | 0.5 GY/BK | 6435 | Can Bus Low Serial Data (LNF) | S | 0.5 GY/BK | 6435 | Can Bus Low Serial Data (LNF)

### X122 Forward Lamp Harness to the Outside Air Temperature Sensor Harness

#### Connector Part Information

- OEM: 12052641
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12162000
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### X122 Forward Lamp Harness to the Outside Air Temperature Sensor Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal | A | 0.5 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal
B | 0.5 YE | 61 | Low Reference | B | 0.5 YE | 61 | Low Reference

### X162 Engine Harness to the Fuel Injector Jumper Harness

#### Connector Part Information

- OEM: 33472-1216
- Description: 12-Way F Sealed (BK)

#### Connector Part Information

- OEM: 33482-1206
- Description: 12-Way M Sealed (BK)

#### X162 Engine Harness to the Fuel Injector Jumper Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1.0 BN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1 | 1 | 1.0 TN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
2 | 1.0 D-BU | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2 | 2 | 1.0 TN | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
3 | 1.0 D-GN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3 | 3 | 1.0 TN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
4 | 1.0 L-BU | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4 | 4 | 1.0 TN | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
5 | 0.5 TN | 808 | Low Reference | 5 | 0.5 GY | 808 | Low Reference
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | 1.0 BN/WH | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1 | 7 | 1.0 TN | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1
8 | 1.0 D-BU/WH | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2 | 8 | 1.0 TN | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2
9 | 1.0 D-GN/WH | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3 | 9 | 1.0 TN | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3
10 | 1.0 L-BU/WH | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4 | 10 | 1.0 TN | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4
11 | 0.5 GY | 598 | 5-Volt Reference | 11 | 0.5 GY | 598 | 5-Volt Reference
12 | 0.5 YE | 2918 | Fuel Rail Pressure Sensor Signal | 12 | 0.5 GY | 2918 | Fuel Rail Pressure Sensor Signal

### X208 SIR I/P Module Harness to the I/P Body Harness

#### Connector Part Information

- OEM: 15336479
- Description: 4-Way F Metri-Pack 280 (YE)

#### Connector Part Information

- OEM: 15336476
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### X208 SIR I/P Module Harness to the I/P Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.5 OG | 3024 | I/P Module - Stage 1 - Low Control | A1 | 0.5 OG | 3024 | I/P Module - Stage 1 - Low Control
A2 | 0.5 YE | 3025 | I/P Module - Stage 1 - High Control | A2 | 0.5 YE | 3025 | I/P Module - Stage 1 - High Control
B1 | 0.5 PU | 3026 | I/P Module - Stage 2 - Low Control | B1 | 0.5 PU | 3026 | I/P Module - Stage 2 - Low Control
B2 | 0.5 GY | 3027 | I/P Module - Stage 2 - High Control | B2 | 0.5 GY | 3027 | I/P Module - Stage 2 - High Control

### X216 I/P Body Harness to the HVAC Harness

#### Connector Part Information

- OEM: 6098-4787
- Description: 8-Way F 2.8 Series (WH)

#### Connector Part Information

- OEM: 6098-4905
- Description: 8-Way M 2.8 Series (WH)

#### X216 Instrument Panel Body Harness to the HVAC Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 2.0 YE | 60 | Blower Motor Low Control | 1 | 2.0 YE | 60 | Blower Motor Low Control
2 | 2.0 TN | 63 | Blower Motor Medium 1 Control | 2 | 2.0 TN | 63 | Blower Motor Medium 1 Control
3 | 2.0 L-BU | 72 | Medium 2 Blower Motor Control | 3 | 2.0 L-BU | 72 | Medium 2 Blower Motor Control
4 | 3.0 OG | 52 | Blower Motor High Control | 4 | 3.0 OG | 52 | Blower Motor High Control
5 | 3.0 BN | 141 | Ignition 3 Voltage | 5 | 3.0 BN | 141 | Ignition 3 Voltage
6 | 3.0 BK | 550 | Ground | 6 | 3.0 BK | 2050 | Ground
7-8 | -- | -- | Not Used | 7-8 | -- | -- | Not Used

### X218 I/P Body Harness to the HVAC Harness

#### Connector Part Information

- OEM: 6098-4789
- Description: 12-Way 1.5 2.8 Series (NA)

#### Connector Part Information

- OEM: 6098-4900
- Description: 12-Way M (WH)

#### X218 Instrument Panel Body Harness to the HVAC Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.35 TN/BK | 2274 | Recirculation Door Control Circuit | 1 | 0.35 TN/BK | 2274 | Recirculation Door Control Circuit
2 | 0.35 D-GN | 1614 | Recirculation Door Control | 2 | 0.35 D-GN | 1614 | Recirculation Door Control
3 | 0.35 D-BU | 1646 | Air Temperature Door Position Signal | 3 | 0.35 D-BU | 1646 | Air Temperature Door Position Signal
4 | 0.35 L-GN | 2275 | Mode Door Position Signal | 4 | 0.35 L-GN | 2275 | Mode Door Position Signal
5 | 0.35 L-GN/BK | 1647 | Air Temperature Door Control | 5 | 0.35 L-GN/BK | 1647 | Air Temperature Door Control
6 | 0.35 L-BU/BK | 1688 | 5-Volt Reference | 6 | 0.35 L-BU/BK | 1688 | 5-Volt Reference
7 | 0.35 L-GN/BK | 2276 | Defrost Door Position Signal | 7 | 0.35 L-GN/BK | 2276 | Defrost Door Position Signal
8 | 0.35 TN | 2273 | Mode Door Control | 8 | 0.35 TN | 2273 | Mode Door Control
9 | 0.35 D-BU | 1199 | Air Temperature Door Control | 9 | 0.35 D-BU | 1199 | Air Temperature Door Control
10 | 0.35 L-BU | 733 | Air Temperature Door Position Signal | 10 | 0.35 L-BU | 733 | Air Temperature Door Position Signal
11 | 0.35 GY | 6137 | Evaporative Emission Core Temperature Sensor Signal (C60) | 11 | 0.35 GY | 6137 | Evaporative Emission Core Temperature Sensor Signal (C60)
12 | 0.35 YE | 1791 | Low Reference | 12 | 0.35 YE | 1791 | Low Reference

### X316 I/P Body Harness to the Passenger Seat Harness

#### Connector Part Information

- OEM: 15332145
- Description: 8-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332150
- Description: 8-Way M GT 150 Series (BK)

#### X316 I/P Body Harness to the Passenger Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal | A | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal
B | -- | -- | Not Used | B | -- | -- | Not Used
C | 0.35 PK | 5057 | Low Reference | C | 0.35 PK | 5057 | Low Reference
D | 0.35 PK | 353 | I/P Module Suppression Indicator Control | D | 0.35 PK | 353 | I/P Module Suppression Indicator Control
E | 0.35 TN/BK | 723 | I/P Module Disable Switch - Signal | E | 0.35 TN | 723 | I/P Module Disable Switch - Signal
F | 0.35 PK | 1339 | Ignition 1 Voltage | F | 0.35 PK | 1339 | Ignition 1 Voltage
G | 0.35 PK | 5018 | Occupant Sensor Serial Data | G | 0.35 PK | 5018 | Occupant Sensor Serial Data
H | 0.5 BK/WH | 351 | Ground | H | 0.5 BK/WH | 351 | Ground

### X317 I/P Body Harness to the Driver Seat Harness

#### Connector Part Information

- OEM: 15326886
- Description: 4-Way F GT280 (BK)

#### Connector Part Information

- OEM: 15326890
- Description: 4-Way M GT280 (BK)

#### X317 Instrument Panel Body Harness to the Driver Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 TN/WH | 238 | Driver Seat Belt Switch Signal | A | 0.35 TN/WH | 238 | Driver Seat Belt Switch Signal
B | 0.35 PK | 5057 | Low Reference | B | 0.35 PK | 5057 | Low Reference
C | 2.0 RD/BK | 642 | Battery Positive Voltage | C | 2.0 RD/BK | 5057 | Battery Positive Voltage (AF2)
D | 2.0 BK | 550 | Ground | D | 2.0 BK | 550 | Ground (AF2)

### X400 I/P Body Harness to the Right Rear Lamp Assembly Harness

#### Connector Part Information

- OEM: E-5651-1
- Description: 6-Way F FTS Series Sealed (L-GY)

#### Connector Part Information

- OEM: E-5655-2
- Description: 6-Way Sealed (D-GN)

#### X400 I/P Body Harness to the Right Rear Lamp Assembly Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 BK | 750 | Ground | 1 | 0.8 BK | 750 | Ground
2 | 0.5 BN | 9 | Tail/License Park Lamps Supply Voltage | 2 | 0.5 BN | 9 | Tail/License Park Lamps Supply Voltage
3 | 0.8 L-GN | 24 | Backup Lamp Supply Voltage | 3 | 0.5 L-GN | 24 | Backup Lamp Supply Voltage
4 | 0.8 L-BU | 20 | Stop Lamp Supply Voltage | 4 | 0.5 L-BU | 20 | Stop Lamp Supply Voltage
5 | 0.5 OG | 122 | Rear Fog Lamp Supply Voltage | 5 | 0.5 OG | 122 | Rear Fog Lamp Supply Voltage
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

### X405 Rear Chassis Harness to Left Rear Lamp Assembly Harness

#### Connector Part Information

- OEM: 6189-0319
- Description: 6-Way F TS Series Sealed (GY)

#### Connector Part Information

- OEM: 6188-0173
- Description: 6-Way M TS 090 Series Sealed (GY)

#### X405 Rear Chassis Harness to Left Rear Lamp Assembly Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 0.8 YE | 618 | Left Rear Turn Signal Lamp Supply Voltage | 2 | 0.8 D-GN | 618 | Left Rear Turn Signal Lamp Supply Voltage
3 | 0.8 D-BU | 809 | Left Tail Lamp Supply Voltage | 3 | 0.8 RD/BU | 809 | Left Tail Lamp Supply Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 0.8 RD | 1050 | Ground | 5 | 0.8 BK | 1050 | Ground
6 | 0.8 L-BU | 20 | Tail/Stop Lamp Supply Voltage | 6 | 0.8 D-GN/WH | 20 | Tail/Stop Lamp Supply Voltage

### X406 I/P Body Harness to Chassis Harness

#### Connector Part Information

- OEM: E-5225-001
- Description: 8-Way F Sealed (BK)

#### Connector Part Information

- OEM: E-5222-003
- Description: 8-Way M Sealed (BK)

#### X406 I/P Body Harness to Chassis Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.5 RD/WH | 140 | Battery Positive Voltage | 1 | 0.5 RD/WH | 140 | Battery Positive Voltage
2 | 0.5 WH | 1310 | Evaporative Emission Canister Vent Solenoid Control | 2 | 0.5 WH | 1310 | Evaporative Emission Canister Vent Solenoid Control
3 | 0.5 PU | 1589 | Fuel Level Sensor Signal | 3 | 0.5 PU | 1589 | Fuel Level Sensor Signal
4 | 1.0 GY | 120 | Fuel Pump Supply Voltage | 4 | 1.0 GY | 120 | Fuel Pump Supply Voltage
5 | 1.0 L-BU | 20 | Stop Lamp Supply Voltage | 5 | 0.8 L-BU | 20 | Stop Lamp Supply Voltage
6 | 0.5 TN | 2759 | Low Reference | 6 | 0.5 TN | 2759 | Low Reference
7 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal | 7 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
8 | 0.5 GY | 2709 | 5-Volt Reference 1 | 8 | 0.5 GY | 2709 | 5-Volt Reference 1

### X407 Rear Chassis Harness to Right Rear Lamp Assembly Harness

#### Connector Part Information

- OEM: 6189-0319
- Description: 6-Way F TS 090 Sealed Series (NA)

#### Connector Part Information

- OEM: 6188-0173
- Description: 6-Way M TS 090 Series Sealed (GY)

#### X407 Rear Chassis Harness to Right Rear Lamp Assembly Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | 0.8 D-GN | 619 | Right Rear Turn Signal Lamp Supply Voltage | 2 | 0.8 D-GN | 619 | Right Rear Turn Signal Lamp Supply Voltage
3 | 0.8 RD | 609 | Right Tail Lamp Supply Voltage | 3 | 0.8 WH | 609 | Right Tail Lamp Supply Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | 0.8 BK | 750 | Ground | 5 | 0.8 BK | 750 | Ground
6 | 0.8 L-BU | 20 | Tail/Stop Lamp Supply Voltage | 6 | 0.8 GN/WH | 20 | Tail/Stop Lamp Supply Voltage

### X408 Chassis Harness to I/P Body Harness

#### Connector Part Information

- OEM: E-5225-001
- Description: 8-Way F Sealed (BK)

#### Connector Part Information

- OEM: E-5222-003
- Description: 8-Way M Sealed (BK)

#### X408 Chassis Harness to I/P Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 BK | 750 | Ground | 1 | 0.8 BK | 750 | Ground
2 | 0.8 TN | 884 | Wheel Speed Sensor Signal - Left Rear (JL9) | 2 | 0.5 TN | 884 | Wheel Speed Sensor Signal - Left Rear (JL9)
3 | 0.8 OG | 885 | Low Reference | 3 | 0.5 OG | 885 | Low Reference
4 | 0.8 BN | 882 | Wheel Speed Sensor Signal - Right Rear (JL9) | 4 | 0.5 BN | 882 | Wheel Speed Sensor Signal - Right Rear (JL9)
5 | 0.8 WH | 883 | Low Reference | 5 | 0.5 WH | 883 | Low Reference
6 | 0.8 YE | 618 | Stop/Turn Lamp Supply Voltage - Left Rear | 6 | 0.8 YE | 618 | Stop/Turn Lamp Supply Voltage - Left Rear
7 | 0.8 D-BU | 809 | Tail Lamp Supply Voltage - Left | 7 | 0.8 D-BU | 809 | Tail Lamp Supply Voltage - Left
8 | 0.8 D-GN | 619 | Stop/Turn Lamp Supply Voltage - Right Rear | 8 | 0.8 D-GN | 619 | Stop/Turn Lamp Supply Voltage - Right Rear

### X409 Chassis Harness to I/P Body Harness

#### Connector Part Information

- OEM: E-5092-001
- Description: 1-Way F Sealed (BK)

#### Connector Part Information

- OEM: E-5096-001
- Description: 1-Way M Sealed (BK)

#### X409 Chassis Harness to I/P Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 WH | 609 | Right Tail Lamp Supply Voltage | 1 | 0.8 WH | 609 | Right Tail Lamp Supply Voltage

### X410 I/P Body Harness to the Rear Lamp Jumper Harness

#### Connector Part Information

- OEM: E-5651-1
- Description: 6-Way F Sealed (BK)

#### Connector Part Information

- OEM: E-5655-2
- Description: 6-Way M Sealed (BK)

#### X410 Instrument Panel Body Harness to the Rear Lamp Jumper Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 0.8 BK | 750 | Ground | 1 | 0.8 BK | 750 | Ground
2 | 0.5 BN | 9 | Park Lamp Supply Voltage | 2 | 0.5 BN | 9 | Park Lamp Supply Voltage
3 | 0.8 L-GN | 24 | Ground | 3 | 0.5 L-GN | 24 | Ground
4 | 0.8 L-BU | 20 | Stop Lamp Supply Voltage | 4 | 0.5 L-BU | 20 | Stop Lamp Supply Voltage
5 | 0.5 OG | 122 | Rear Fog Lamp Supply Voltage | 5 | 0.5 OG | 122 | Rear Fog Lamp Supply Voltage
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

### X500 Driver Door Harness to the I/P Body Harness

#### Connector Part Information

- OEM: 15326842
- Description: 10-Way F 150 Sealed (BK)

#### Connector Part Information

- OEM: 15326847
- Description: 10-Way M 150 Sealed (BK)

#### X500 Driver Door Harness to the I/P Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.8 GY | 118 | Left Front Speaker Output (-) | A | 1.0 GY (UQ3) | 118 | Left Front Speaker Output (-)
0.8 GY (UW5)
B | 0.8 TN | 201 | Left Front Speaker Output (+) | B | 1.0 TN (UQ3) | 201 | Left Front Speaker Output (+)
0.8 TN (UW5)
C | 0.5 GY | 295 | Door Lock Actuator Lock Control (AU3) | C | 0.5 GY | 295 | Door Lock Actuator Lock Control (AU3)
D | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control (AU3/AU0) | D | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control (AU3/AU0)
D | 0.5 GY | 550 | Ground (without AU3) | D | 0.5 GY | 550 | Ground (without AU3)
E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (D48) | E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (D48)
F | 0.35 OG/WH | 881 | Passenger Mirror Motor Left Control (D48) | F | 0.35 OG/WH | 881 | Passenger Mirror Motor Left Control (D48)
G | 0.35 PU/WH | 889 | Passenger Mirror Motor Left/Down Control | G | 0.35 PU/WH | 889 | Passenger Mirror Motor Left/Down Control
H | 0.35 TN/WH | 330 | Right Mirror Motor Supply Voltage (D48) | H | 0.35 TN/WH | 330 | Right Mirror Motor Supply Voltage (D48)
J | 0.35 RD/WH | 440 | Battery Positive Voltage (D48) | J | 0.35 RD/WH | 440 | Battery Positive Voltage (D48)
K | 0.35 GY/BK | 745 | Driver Door Ajar Switch Signal | K | 0.35 GY/BK | 745 | Driver Door Ajar Switch Signal

### X501 Driver Door Harness to the I/P Body Harness (A31)

#### Connector Part Information

- OEM: 15326654
- Description: 8-Way F GT 280 Series Sealed 5.8 (BK)

#### Connector Part Information

- OEM: 15326655
- Description: 8-Way M GT 280 Series Sealed 5.8 (BK)

#### X501 Driver Door Harness to the I/P Body Harness (A31)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal | A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal
B | 2.0 BK | 550 | Ground | B | 2.0 BK | 550 | Ground
C | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage | C | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal | D | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal
E | 1.0 RD/WH | 240 | Battery Positive Voltage | E | 1.0 RD/WH | 240 | Battery Positive Voltage
F | 0.5 WH | 682 | Door Lock Lock/Unlock Signal | F | 0.35 BN | 682 | Door Lock Lock/Unlock Signal
G-H | -- | -- | Not Used | G-H | -- | -- | Not Used

### X505 Driver Door Harness to the Power Mirror Jumper Harness

#### Connector Part Information

- OEM: 15332153
- Description: 10-Way F 150 Sealed (BK)

#### Connector Part Information

- OEM: 15332158
- Description: 10-Way M 150 Sealed (BK)

#### X505 Driver Door Harness to the Power Mirror Jumper Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | 0.35 BK | 550 | Ground | B | 0.35 BK | 550 | Ground
C | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage | C | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage
D | 0.35 WH | 81 | Driver Mirror Motor Right Control | D | 0.35 WH | 81 | Driver Mirror Motor Right Control
E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage | E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
F | 0.35 L-GN | 89 | Driver Mirror Motor Down Control | F | 0.35 L-GN | 89 | Driver Mirror Motor Down Control
G | 0.35 RD/WH | 440 | Battery Positive Voltage | G | 0.35 RD/WH | 440 | Battery Positive Voltage
H | 0.35 TN | 329 | Driver Mirror Motor Supply Voltage | H | 0.35 TN | 329 | Driver Mirror Motor Supply Voltage
J | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control | J | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control
K | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control | K | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control

### X600 Passenger Door Harness to the I/P Body Harness

#### Connector Part Information

- OEM: 15326084
- Description: 16-Way F GT 150 280 Series Sealed 4.0 5.8 (BK)

#### Connector Part Information

- OEM: 15326085
- Description: 16-Way M GT 150 280 Series Sealed 4.0 5.8 (BK)

#### X600 Passenger Door Harness to the I/P Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31) | A | 3.0 L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31)
B | 0.8 D-GN | 117 | Right Front Speaker Output (-) | B | 1.0 D-GN | 117 | Right Front Speaker Output (-)
C | 0.8 L-GN | 200 | Right Front Speaker Output (+) | C | 1.0 L-GN | 200 | Right Front Speaker Output (+)
D | 0.5 TN | 294 | Door Lock Actuator Unlock Control (AU3/AU0) | D | 0.5 TN | 294 | Door Lock Actuator Unlock Control (AU3/AU0)
E | 0.5 GY | 295 | Door Lock Actuator Lock Control (AU3/AU0) | E | 0.5 GY | 295 | Door Lock Actuator Lock Control (AU3/AU0)
F | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (D48) | F | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (D48)
G | 0.35 OG/WH | 881 | Passenger Mirror Motor Left Control (D48) | G | 0.35 OG/WH | 881 | Passenger Mirror Motor Left Control (D48)
H | -- | -- | Not Used | H | -- | -- | Not Used
J | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage (A31) | J | 3.0 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage (A31)
K | 0.35 BN/WH | 889 | Passenger Mirror Motor Left/Down Control (D48) | K | 0.35 PU/WH | 889 | Passenger Mirror Motor Left/Down Control (D48)
L | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage (D48) | L | 0.35 TN/WH | 330 | Passenger Mirror Motor Supply Voltage (D48)
M | 0.5 WH | 682 | Door Lock Lock/Unlock Signal | M | 0.35 YE | 682 | Door Lock Lock/Unlock Signal
N | 0.35 TN/WH | 746 | Passenger Door Ajar Switch Signal | N | 0.35PKN/WH | 746 | Passenger Door Ajar Switch Signal
P | 0.35 BK | 550 | Ground | P | 0.5 BK | 550 | Ground
R | -- | -- | Not Used | R | -- | -- | Not Used
S | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal (A31) | S | 3.0 TN | 167 | Power Window Master Switch Right Front Down Signal (A31)