For 1990-2009 cars

### Removal Procedure

1. Remove the starter. Refer to Starter Motor Replacement.
2. Disconnect the engine wiring harness electrical connector (1) from the crankshaft position (CKP) sensor.
3. Remove the CKP sensor bolt.
4. Remove the CKP sensor.

### Installation Procedure

1. Lubricate the CKP sensor O-ring seal with clean engine oil.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the CKP sensor.
3. Install the CKP sensor bolt and tighten to 10 N·m (89 lb in).
4. Connect the engine wiring harness electrical connector (1) to the CKP sensor.
5. Install the starter. Refer to Starter Motor Replacement.