For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the intake manifold cover. Refer to Intake Manifold Cover Replacement .
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
3. Remove the power steering pump pulley. Refer to Power Steering Pump Pulley Replacement .

1 | Power Steering Fluid Reservoir Outlet Hose Clamp

#### Procedure

Remove as much power steering fluid as possible from the remote power steering fluid reservoir.

2 | Power Steering Fluid Reservoir Outlet Hose
3 | Power Steering Gear Inlet Hose Fitting Notice: Refer to Fastener Notice in the Preface section. Tighten 27 N·m (20 lb ft)
4 | Power Steering Pump Bolt (Qty: 3) Tighten 22 N·m (16 lb ft)
5 | Power Steering Pump

#### Procedure

1. Remove the power steering pump from the top of the vehicle.
2. Fill and bleed the power steering system. Refer to Power Steering System Bleeding .