For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the brake cooling duct retainer.

1 | Front Fascia Retainers (Qty: 12)
2 | Front Fascia Screws (Qty: 22) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Front Fascia Bracket Screws (Qty: 4) Tighten 2 N·m (18 lb in)
4 | Front Fascia Center Bracket Retainers
5 | Front Fascia Tip Disconnect the lamp connectors.