For 1990-2009 cars
Battery Voltage: The scan tool displays Normal/Out of Range. This is the current battery voltage available at the body control module (BCM) with normal being between 9 and 16 volts.
Door Ajar Switch: The scan tool displays Door Closed/Door Ajar. The passenger door ajar switch input to the BCM, where an open door is displayed as Door Ajar.
Door Lock Switch: The scan tool displays Voltage.
Door Lock Switch: The scan tool displays Idle/Lock/Unlock. This is the state of the driver and passenger door lock switches.
Driver Door Ajar Sw.: The scan tool displays Door Closed/Door Ajar. The driver door ajar switch input to the BCM, where an open door is displayed as Door Ajar.
Driver Door Lock Actuator Command: The scan tool displays Idle/Lock/Unlock/Invalid. The state of the driver door lock actuator output.
Passenger Doors Lock Actuator Command: The scan tool displays Idle/Lock/Unlock/Invalid. The state of the passenger door lock actuators outputs.
Trunk Ajar Switch: The scan tool displays the status of the trunk ajar switch.
Trunk Motor: The scan tool displays the current state of the trunk release motor.
Trunk Release Solenoid Command: The scan too displays the status of the truck release solenoid output control.
Trunk Release Switch: The scan tool displays the status of the trunk release switch input.