For 1990-2009 cars

Table 1: | Body Control Module (BCM)
Table 2: | Instrument Panel Cluster (IPC)
Table 3: | Engine Control Module (ECM)

The scan tool data lists contain all the instrument panel, gages, and console related parameters that are available on the scan tool. The parameters in the list are arranged in alphabetical order. The data list column indicates the location of the parameter within the scan tool menu selections.

Use the scan tool data lists as directed by a diagnostic table or in order to supplement the diagnostic procedures. Begin all of the diagnostic procedures with the Diagnostic System Check - Vehicle .

Use the scan tool data lists only after the following is determined:

• | There is no published DTC procedure nor published symptom procedure for the customer concern.

• | The DTC or symptom procedure indicated by the diagnostic system check does not resolve the customer concern.

The typical data values are obtained from a properly operating vehicle under the conditions specified in the first row of the scan tool data list table. Comparison of the parameter values from the suspect vehicle with the typical data values may reveal the source of the customer concern.

#### Body Control Module (BCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF/Seat Belt Buckled/High Beams OFF/Park Brake Unapplied
Ambient Air Temp. Sensor | HVAC Data | Volts | Varies
Battery Voltage Signal | Keyless/Remote Start Data | Volts | Varies
Brake Fluid Level Sensor | Chassis Data | Low/OK | OK
DIC Switch | Chassis Data | Clear/Menu/Info/Reset | Clear
Driver Door Ajar Switch | Keyless/Remote Start Data | Door Closed/Door Ajar | Door Closed
Key In Ignition Cylinder Switch | Keyless/Remote Start Data | Yes/No | Yes
Headlamp Off Switch | Lighting Data | Off/On | Off
Headlamp On Switch | Lighting Data | Off/On | Off
Park Lamp Switch | Lighting Data | Off/On | Off
Trunk Ajar Switch | Keyless/Remote Start Data | Trunk Closed/Trunk Ajar | Trunk Closed

#### Instrument Panel Cluster (IPC)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF/Seat Belt Buckled/High Beams OFF/Park Brake Unapplied
Battery Voltage Signal | IPC Data | Volts | Varies
DIC Information Switch | IPC Data | Inactive/Active | Inactive
DIC Switch Input | IPC Data | Volts | Varies
Ignition 1 Input | IPC Data | Inactive/Active | Active
Menu Switch | IPC Data | Off/On | Off
Reset Switch | IPC Data | Inactive/Active | Inactive

#### Engine Control Module (ECM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Engine Idling/Normal Operating Temperature
Cruise Control Active | ECM IPC Data | Yes/No | No
ECT Sensor | ECM IPC Data | Celsius (Fahrenheit) | Varies 8 -105°C (185-220°F)
Engine Oil Level Switch | ECM IPC Data | OK/Low | OK
Engine Oil Pressure Switch | ECM IPC Data | OK/Low | OK
Engine Oil Temperature Calculated | ECM Data | Celsius (Fahrenheit) | Varies w/oil temperature
Engine Speed | ECM IPC Data | RPM | ±100 RPM from Desired Idle Speed
Fuel Level Sensor | ECM IPC Data | Volts | 0-5 Volts Varies w/fuel level
Fuel Tank Level Remaining | ECM IPC Data | Percent (%) | 0-100% Varies w/fuel level
Ignition Accessory Signal | ECM IPC Data | On/Off | Off
Ignition 1 Signal | ECM IPC Data | Volts | 9-16 Volts Varies
MIL Command | ECM IPC Data | On/Off | Off
Non-Driven Wheel Speed | ECM IPC Data | km/h (mph) | 0 km/h (0 mph)
Odometer | ECM IPC Data | kilometers (miles) | Varies
Reduced Engine Power | ECM IPC Data | Inactive/Active | Inactive
Vehicle Speed Sensor | ECM IPC Data | km/h (mph) | 0 km/h (0 mph)