For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear bumper extension. Refer to Rear Bumper Extension Replacement.
2. Disconnect the electrical harness connector from the tab on the rear bumper valance center panel.
3. Remove the two lower backup lamp screws from the rear bumper valance center panel.

1 | Backup Lamp Assembly Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Backup Lamp Assembly Tip Replace or transfer the bulbs as needed.