For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Brake Dust Caution in the Preface section. Caution: Refer to Brake Fluid Irritant Caution in the Preface section.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .

1 | Brake Pipe Fitting Notice: Refer to Fastener Notice in the Preface section. Tip Cap the brake pipe fitting to prevent brake fluid loss and contamination. Tighten
20 N·m (15 lb ft)

2 | Brake Hose Bracket Bolt Tighten 12 N·m (106 lb in)
3 | Brake Hose Fitting Bolt Tighten 40 N·m (30 lb ft)
4 | Brake Hose Fitting Gasket (Qty: 2) Tip DO NOT reuse the brake hose fitting gaskets. Install NEW gaskets.
5 | Front Brake Hose

#### Procedure

Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding .