For 1990-2009 cars

### Removal Procedure

1. Remove the turbocharger. Refer to Turbocharger Replacement .
2. Remove the exhaust manifold heat shield bolts.
3. Remove the exhaust manifold heat shield.

### Installation Procedure

1. Install the exhaust manifold heat shield.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the exhaust manifold heat shield bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Install the turbocharger. Refer to Turbocharger Replacement .