For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Driver and Passenger Seat Replacement .
2. Remove the seat back recliner handle. Refer to Driver Seat and Passenger Seat Recliner Handle Replacement .
3. Remove the seat back recliner cover. Refer to Front Seat Back Recliner Outer Trim Panel Replacement .

1 | Seat Cushion Frame Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tip Fold the seat back forward to access the bolts. Tighten
25 N·m (18 lb ft)

2 | Seat Outer Adjuster Assembly
3 | Seat Adjuster Handle Assembly Refer to Two-Way Manual Seat Adjuster Handle Replacement .
4 | Seat Adjuster Retaining Spring
5 | Seat Belt Buckle Bolt Tighten 45 N·m (33 lb ft)
6 | Seat Belt Buckle Assembly

#### Procedure

Disconnect the electrical connectors.

7 | Seat Cushion Frame Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
8 | Seat Inner Adjuster Assembly

#### Procedure

Pull up on the adjuster handle and synchronize both the inner and outer adjuster assembly into the same position.